**Comparative Statement for “Work of White Washing & Painting of Electronics Trade (Block –B) At Govt. ITI Solan (H.P.)”Opened on Dated 29/11/2023 at 03:30 PM.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr. No/code** | | **Particulars of Items** | **Unit** | **Qty. Req.  in Units** | **M/s Prem Chauhan Contractor** | **M/s Ram Prakash Govt. & Private Contractor** | **M/s Kunal Sahni Contractor** |
| 1 | 13.88 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete Walls. | Sqm | 314.10 | 2512.8 | 2764.08 | 2826.9 |
| 2 | 14.1 | Repairs to plaster of thickness 12mm to 20mm in patches of area 2.5 sq. mtrs and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground , all complete as per direction of Engineer – in charge.  14.1.1 with cement mortar 1:4 (1 Cement : 4 Fine Sand) | Sqm | 219.43 | 57051.8 | 59026.67 | 59246.1 |
| 3 | 13.26 | Providing and applying plaster of parts putty of 2mm thickness over plastered surface to prepare the surface even and smooth.  Putty only Required Surfaces | Sqm | 219.43 | 28745.33 | 29842.48 | 29623.05 |
| 4 | 13.90 | Distempering with 1st quality acrylic distemper (ready mix ) having VOC content less than 50 grams/ litre of approved brand and manufacture to give an even shade :  13.90.1 old work (one or more coats ) | Sqm | 274.29 | 10423.02 | 13988.79 | 10971.6 |
| 5 | 13.48 | 13.48.2: Painting wood work with deluxe multi surface paint of required shade.: Two or more coats applied @ of 0.90 ltr/10 sqm over and under coat of primer applied @ 0.75 ltr/10sqm of approved brand and manufacture. Doors Window and Walls | Sqm | 39.81 | 3702.33 | 4578.15 | 3702.33 |
| 6 | 13.48 | Finishing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications  13.48.3 Painting Steel work with Deluxe Multi Surface Paint to give an even shade. Two or more coat applied @ 0.90 ltr/ 10 sqm over an under coat of primer applied @ 0.80 ltr/ 10 sqm of approved brand and manufacture  **Enamd on steel paint** | Sqm | 25.74 | 2316.6 | 2316.6 | 2316.6 |
| 7 | 13.51 | Painting with silicon & acrylic emulsion based water thinable sealer of approved brand and manufacture on wet patchy portion of plastered surface.  13.51.2 Two Coated | Sqm | 30.82 | 1787.56 | 1880.02 | 1910.84 |
|  |  | **Grand Total** | | | 106539.40 | 114396.80 | 110597.40 |

Certified that rates/amount quoted by **M/s Prem Chauhan C/O Jaggi Niwas, Near ITI Solan, Kather Bye Pass Solan (H.P.)** are found lowest, hence recommended for approval please.

1. Store Keeper 2. Civil Expert 3. Store Officer 4. Concerned G.I. 5. Industry member

Member Secy. IMC cum Principal (Sr-Scale)

Govt. ITI (Grade-A) Solan (HP)

Chairman

Works and procurement committee (IMC) Govt. ITI (Grade A) Solan (HP)