**Tender Form (Financial Bid)**

To

 Member Secy., IMC for ITI Solan

 cum Principal, Govt. ITI Solan

 Distt. Solan HP-173212

**Sub: - Internal Estimate for White Washing& Painting of:-**

**A)- Mess In Boys Hostel At Govt. ITI Solan ( H.P) Annaxure - I**

|  |  |
| --- | --- |
| **Name of Bidder** |  |
| **Address of the Bidder** |  |
| **Sr. No/code** | **Particulars of Items** | **Unit** | **Qty. Req. in Units** | **Rate Per Unit in Rs. In Figures *(Excluding GST)*** | **Rate Per Unit in Rs. In Words *(Excluding GST)*** | **Amount in Rs. In Figures *(Excluding GST)*** |
|  |  | **Particulars of Item** |  |  |  |  |  |
| 1 | 13.88 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete Walls.  | Sqm | 344.82 |  |  |  |
| 2 | 14.1 | Repairs to plaster of thickness 12mm to 20mm in patches of area 2.5 sq.mtrs and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground , all complete as per direction of Engineer – in charge.14.1.1 with cement mortar 1:4 (1 Cement : 4 Fine Sand) | Sqm | 113.08 |  |  |  |
| 3 | 13.26 | Providing and applying plaster of parts putty of 2mm thickness over plastered surface to prepare the surface even and smooth.Putty only Required Surfaces | Sqm | 113.08 |  |  |  |
| 4 | 13.81 | Distempering with 1st quality acrylic distemper, having VOC (Volatile Organic Compound ) content less than 50 grams/ litre, of approved brand and manufacture, including applying additional coats wherever required, to achieve even shade and colour**13.81.2** Two coats and more |  Sqm | 323.10 |  |  |  |
| 5 | 11.41 | providing and laying vitrified floor tiles in different sizes (thickness to be specified by the manufacturer) with water absorption less than 0.08% and conforming to IS: 15622, of approved make, in all colours and shades, laid on 20mm thick cement mortar 1:4 (1 cement : 4 coarse sand), jointing with grey cement slurry @ 3.3 kg/ sqm including grouting the joints with white cement and matching pigments etc., complete **11.41.1** Size of Tile 500x500 mm | Sqm | 70.00 |  |  |  |
| 6 | 13.48 | Finishing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.2: Painting wood work with deluxe multi surface paint of required shade.: Two or more coats applied @ of 0.90 ltr/10 sqm over and under coat of primer applied @ 0.75 ltr/10sqm of approved brand and manufacture. Doors Window and Walls  | Sqm | 21.72 |  |  |  |
| 7 | 13.48 | Finishing with Deluxe Multi surface paint system for interiors and exteriors using Primer as per manufacturers specifications :13.48.3 Painting Steel work with Deluxe Multi Surface Paint to give an even shade. Two or more coat applied @ 0.90 ltr/ 10 sqm over an under coat of primer applied @ 0.80 ltr/ 10 sqm of approved brand and manufacture | Sqm | 21.72 |  |  |  |

**B) - Plumber Trade (Block-D) Annaxure-II**

|  |  |
| --- | --- |
| **Name of Bidder** |  |
| **Address of the Bidder** |  |
| **Sr. No/code** | **Particulars of Items** | **Unit** | **Qty. Req. in Units** | **Rate Per Unit in Rs. In Figures *(Excluding GST)*** | **Rate Per Unit in Rs. In Words *(Excluding GST)*** | **Amount in Rs. In Figures *(Excluding GST)*** |
|  |  | **Particulars of Item** |  |  |  |  |  |
| 8 | 13.88 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete Walls.  | Sqm | 197.03 |  |  |  |
| 9 | 14.1 | Repairs to plaster of thickness 12mm to 20mm in patches of area 2.5 sq.mtrs and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground , all complete as per direction of Engineer – in charge.14.1.1 with cement mortar 1:4 (1 Cement : 4 Fine Sand) | Sqm | 96.78 |  |  |  |
| 10 | 13.26 | Providing and applying plaster of parts putty of 2mm thickness over plastered surface to prepare the surface even and smooth.Putty only Required Surfaces | Sqm | 96.78 |  |  |  |
| 11 | 13.90 | Distempering with 1st quality acrylic distemper (ready mix ) having VOC content less than 50 grams/ litre of approved brand and manufacture to give an even shade : 13.90.1 old work (two coats )  |  Sqm | 186.13 |  |  |  |
| 12 | 13.48 | 13.48.2: Painting wood work with deluxe multi surface paint of reruired shade.: Two or more coats applied @ of 0.90 ltr/10 sqm over and under coat of primer applied @ 0.75 ltr/10sqm of approved brand and manufacture. Doors Window and Walls  | Sqm | 10.90 |  |  |  |
| 13 | 13.48 | Finshing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.3 Painting Steel work with Deluxe Multi Surface Paint to give an even shade. Two or more coat applied @ 0.90 ltr/ 10 sqm over an under coat of primer applied @ 0.80 ltr/ 10 sqm of approved brand and manufacture**Enamd on steel paint** | Sqm | 3.96 |  |  |  |
| 14 | 13.51 | Finshing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.1: Two or more coats applied on walls @ 1.25 ltr/10 sqm over and including one coat of Special primer applied @0.75ltr/10sqm. | Sqm | 29.82 |  |  |  |

**C) - Sewing Technology Trade (Block-A) Annaxure - III**

|  |  |
| --- | --- |
| **Name of Bidder** |  |
| **Address of the Bidder** |  |
| **Sr. No/code** | **Particulars of Items** | **Unit** | **Qty. Req. in Units** | **Rate Per Unit in Rs. In Figures *(Excluding GST)*** | **Rate Per Unit in Rs. In Words *(Excluding GST)*** | **Amount in Rs. In Figures *(Excluding GST)*** |
|  |  | **Particulars of Item** |  |  |  |  |  |
| 15 | 13.88 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete Walls.  | Sqm | 263.86 |  |  |  |
| 16 | 14.1 | Repairs to plaster of thickness 12mm to 20mm in patches of area 2.5 sq.mtrs and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground , all complete as per direction of Engineer – in charge.14.1.1 with cement mortar 1:4 (1 Cement : 4 Fine Sand) | Sqm | 52.41 |  |  |  |
| 17 | 13.26 | Providing and applying plaster of parts putty of 2mm thickness over plastered surface to prepare the surface even and smooth.Putty only Required Surfaces | Sqm | 52.41 |  |  |  |
| 18 | 13.90 | Distempering with 1st quality acrylic distemper (ready mix ) having VOC content less than 50 grams/ litre of approved brand and manufacture to give an even shade : 13.90.1 old work (one or more coats )  | Sqm | 238.27 |  |  |  |
| 19 | 13.48 | 13.48.2: Painting wood work with deluxe multi surface paint of reruired shade.: Two or more coats applied @ of 0.90 ltr/10 sqm over and under coat of primer applied @ 0.75 ltr/10sqm of approved brand and manufacture. Doors Window and Walls  | Sqm | 25.59 |  |  |  |
| 20 | 13.48 | Finshing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.3 Painting Steel work with Deluxe Multi Surface Paint to give an even shade. Two or more coat applied @ 0.90 ltr/ 10 sqm over an under coat of primer applied @ 0.80 ltr/ 10 sqm of approved brand and manufacture**Enamd on steel paint** | Sqm | 25.59 |  |  |  |

**GST as applicable will be paid extra.**

 Signature of Bidder with

 Date & Seal