**Comparative Statement for “Work of White Washing And Painting at Fitter Trade of Govt. ITI Solan.” Opened on Dated 20/09/2023 at 10:45AM.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr.****No./code** | **Description of Sub head/ Item of work** | **Qty** | **Unit** | **M/s ram Prakash****Near Harsh Palace Hotel****Bypass Kather Solan (HP)** | **M/s Viyom Siddharth****(Decoracio)By pass road Saproon near KFC solan HP** | **M/S Deepak Singh Vill. Anji P.O. Barog Teh. Distt. Solan (H.P)** | **Remarks** |
| 1/13.88 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc. complete  | 215.14 | Sqm | 860 | 12900 | 645.42 |  |
| 2/14.1 | Repairs to plaster of thickness 12mm to 20mm in patches of area 2.5 sq.mtrs and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete, including disposal of rubbish to the dumping ground , all complete as per direction of Engineer – in charge.14.1.1 with cement mortar 1:4 (1 Cement : 4 Fine Sand) | 303.04 | Sqm | 45456 | 119700 | 21212.8 |  |
| 3/13.26 | Providing and applying plaster of parts putty of 2mm thickness over plastered surface to prepare the surface even and smooth.Putty only Required Surfaces | 303.04 | Sqm | 16667.20 | 12120 | 12121.60 |  |
|  4/13.90 | Distempering with 1st quality acrylic distemper, having VOC (Volatile Organic Compound ) content less than 50 grams/ litre, of approved brand and manufacture, including applying additional coats wherever required, to achieve even shade and colour. 13.90.1 (one or more coats) | 378.80 | Sqm | 9091.20 | 22730 | 15152 |  |
| 5/13.48 | Finshing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.1 : Two or more coats applied on walls @ 1.25 ltr/10 sqm over and including one coat of special primer applied @ 0.75 ltr/10sqm. | 53.64 | Sqm | 3218.4 | 4020 | 2682 |  |
| 6/13.48 | 13.48.2: Painting wood work with deluxe multi surface paint of reruired shade.: Two or more coats applied @ of 0.90 ltr/10 sqm over and under coat of primer applied @ 0.75 ltr/10sqm of approved brand and manufacture.Doors window and walls.  | 48.60 | Sqm | 2430 | 6300 | 2187 |  |
| 7/13.48 | Finshing with deluxe multi surface paint system for interiors and exteriors using primer as per manufacturers specifications 13.48.3 Painting Steel work with Deluxe Multi Surface Paint to give an even shade. Two or more coat applied @ 0.90 ltr/ 10 sqm over an under coat of primer applied @ 0.80 ltr/ 10 sqm of approved brand and manufacture**Enamd on steel paint** | 48.60 | Sqm | 2430 | 4130 | 2430 |  |
| 8/14.6 | Renewing glass panes, with wooden fillets wherever necessary: 14.6.1 Float glass panes of nominal thickness 4 mm (weight not less than 10kg/sqm.) | 0.80 | Sqm | 400 | 1000 | 720 |  |
|  | **TOTAL** |  |  | 80552.8 | 182900 | **57150.82** |  |

Certified that rates/amount quoted by **M/S Deepak Singh Vill. Anji P.O. Barog Teh. Distt. Solan (H.P)** are found lowest, hence recommended for approval please.

1. Store Keeper 2. Civil Expert 3. Store Officer 4. Concerned G.I. 5. Industry member Member Secy. IMC Cum

 Principal (Sr. Scale)

 Govt. ITI(Grade A) Solan.

 Chairman

 Works and procurement committee (IMC)