**Comparative Statement for “Work of Kota Stone in Floor at Fitter Trade of Govt. ITI Solan.” Opened on Dated 07/10/2023 at 10:45AM.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Sr.****No./code** | **Description of Sub head/ Item of work** | **Qty** | **Unit** | **Vikrant Sharma****Vill dakeher, p.o. & tehsil jubbal Distt. Shima. (H.P)** | **Dalip singh Thakur, jeevan deep niwas, below BCS new Shimla, Shimla** | **M/S Deepak Singh Vill. Anji P.O. Barog Teh. Distt. Solan (H.P)** | **Remarks** |
| 2/3.4 | cement mortar 1:4 (1 cement : 4 fine sand) | **28.2** | Cum | 53,439 | 69,090 | 42,300 |  |
| 3/11.26 | Kota stone slab flooring over 20 mm (average) thick base laid over and jointed with grey cement slurry mixed with pigment to match the shade of the slab, including rubbing and polishing complete with base of cement mortar 1 : 4 (1 cement : 4 coarse sand) :11.26.1 25 mm thick  | **141.2** | Sqm | 1,57,438 | 1,68,734 | 1,34,846 |
| 4/11.27 | Kota stone slabs 20 mm thick in risers of steps, skirting, dado and pillars laid on 12 mm (average) thick cement mortar 1:3 (1 cement: 3 coarse sand) and jointed with grey cement slurry mixed with pigment to match the shade of the slabs, including rubbing and polishing complete. Long Wall Short Wall | **7.62** | Sqm | 8,801.10 | 9,829.80 | 7,277.10 |
|  |  **TOTAL:-** |  |  | 2,19,678.10 | 2,47,653.80 | **1,84,423.10** |  |

Certified that rates/amount quoted by **M/S Deepak Singh Vill. Anji P.O. Barog Teh. Distt. Solan (H.P)** are found lowest, hence recommended for approval please.

1. Store Keeper 2. Civil Expert 3. Store Officer 4. Concerned G.I. 5. Industry member Member Secy. IMC Cum

 Principal (Sr. Scale)

 Govt. ITI(Grade A) Solan.

 Chairman

 Works and procurement committee (IMC)