**Tender Form (Financial Bid)**

**To**

To

The Member Secy., IMC for ITI Solan

cum Principal, Govt. ITI Solan

Distt. Solan HP-173212

**Sub:- Submission of financial bid of Work of Kota Stone in Floor at Fitter Trade of Govt. ITI Solan**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Name of Bidder** | | |  | | | | | |
| **Address of the Bidder** | | |  | | | | | |
| **Sr. No.** | **Code No.** | **Particulars of Items** | | **Unit** | **Qty. Req.  in Units** | **Rate Per Unit in Rs. In Figures *(Excluding GST)*** | **Rate Per Unit in Rs. In Words *(Excluding GST)*** | **Amount in Rs. In Figures *(Excluding GST)*** |
|  |  | **Particulars of Item** | |  |  |  |  |  |
| 1 | 3.4 | cement mortar 1:4 (1 cement : 4 fine sand) | | Cum | **28.2** |  |  |  |
| 2 | 11.26 | Kota stone slab flooring over 20 mm (average) thick base laid over and jointed with grey cement slurry mixed with pigment to match the shade of the slab, including rubbing and polishing complete with base of cement mortar 1 : 4 (1 cement : 4 coarse sand) :11.26.1 25 mm thick | | Sqm | **141.2** |  |  |  |
| 3 | 11.27 | Kota stone slabs 20 mm thick in risers of steps, skirting, dado and pillars laid on 12 mm (average) thick cement mortar 1:3 (1 cement: 3 coarse sand) and jointed with grey cement slurry mixed with pigment to match the shade of the slabs, including rubbing and polishing complete. Long Wall Short Wall | | Sqm | **7.62** |  |  |  |

**GST as applicable will be paid extra**

Signature of Bidder with

Date & Seal